|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | | | |
| **PARTS** | | | |
|  | | | |
| **ID** | **Description** | **QTY** | |
| 1 | PVC Pipe, ½”, 25 mm length | 7 | |
| 2 | PVC Pipe, ½”, 30 mm length | 3 | |
| 3 | PVC Pipe, ½”, 60 mm - xx mm length | 2 | |
| 4 | PVC Union, ½” Soc x ½” Soc | 1 | |
| 5 | PVC Elbow, ½” Soc x ½” Soc | 6 | |
| 6 | PVC Tee, ½” Soc x ½” Soc x ½” Soc | 3 | |
| 7 | PVC Adapter, ½” NPT x ½” Female Soc Adapter | 1 | |
| 8 | C-Clamp, 2-1/2” | 2 | |
| **TOOLS AND SUPPLIES** | | |
|  | | |
| **Description** | | |
| PVC Cutters OR Hacksaw | | |
| PVC Cement (Optional) | | |

|  |  |  |  |
| --- | --- | --- | --- |
|  | |  | |
| **01.** | **Use the PVC cutters or hacksaw to cut the PVC pipe to length.** | **02.** | **Insert two short PVC sections into an elbow.** |
|  | |  | |
| **03.** | **Insert an elbow onto each pipe section.** | **04.** | **Repeat Steps 2 and 3 to create a second side.** |
|  | |  | |
| **05.** | **Insert longer PVC section into elbows.** | **06.** | **Connect second side.** |
|  | |  | |
| **07.** | **(Optional) Use pencil to mark lines across joints.** | **08.** | **(Optional) Disassemble and reassemble with PVC cement. Erase pencil marks.** |