|  |  |  |  |
| --- | --- | --- | --- |
|  | | | |
| **PARTS** | | |
| 2  1  3  1  2  2  3  1  1  2  1  1 | | |
| **ID** | **Description** | **QTY** |
| 1 | PVC Elbow 90 deg, ½” | 6 |
| 2 | PVC Pipe, ½”, 30 mm length | 4 |
| 3 | PVC Pipe, ½”, 30 mm OR 70 mm for use with Quick Clamp | 2 |

|  |
| --- |
| **TOOLS AND SUPPLIES** |
|  |
| **Description** |
| PVC Cutters OR Hacksaw |
| PVC Cement (Optional) |

|  |  |  |  |
| --- | --- | --- | --- |
|  | |  | |
| **01.** | **Use the PVC cutters or hacksaw to cut the PVC pipe to length.** | **02.** | **Insert two short PVC sections into an elbow.** |
|  | |  | |
| **03.** | **Insert an elbow onto each pipe section.** | **04.** | **Repeat Steps 2 and 3 to create a second side.** |
|  | |  | |
| **05.** | **Insert longer PVC section into elbows.** | **06.** | **Connect second side.** |
|  | |  | |
| **07.** | **(Optional) Use pencil to mark lines across joints.** | **08.** | **(Optional) Disassemble and reassemble with PVC cement. Erase pencil marks.** |